# ADC ft. PWM

Code from a make-up assignment.

Pin layout:

5v out --> variable resistor --> PA1 **(ADC)**

PE14 --> LED --> gnd **(PWM)**

PA11 --> LED + Resistor --> gnd **(optional, "ON" light)**

PA12 --> LED + Resistor --> gnd **(optional, "ERR" light)**

---

To use UART on linux:
- install `minicom` with your package manager
- run `./uart.sh`

